

**REPORT ON AUTOMATED WHEELCHAIR WITH FALL DETECTION**

**Title: Report on Automated Wheelchair with Fall Detection**

**1. Executive Summary:** This report provides an in-depth analysis of an automated wheelchair equipped with fall detection technology. The integration of fall detection capabilities in automated wheelchairs aims to enhance user safety and provide immediate assistance in case of an accident.

**2. Introduction:** Automated wheelchairs have revolutionized mobility for individuals with limited mobility. The incorporation of fall detection technology adds an extra layer of safety, addressing concerns related to accidental falls and their potential consequences.

**3. Objectives:** The primary objectives of the automated wheelchair with fall detection are:

* Enhancing user safety and reducing the risk of injuries.
* Providing timely assistance in the event of a fall.
* Improving the overall user experience and independence.

**4. Features of the Automated Wheelchair:**

**4.1 Automated Mobility:** The wheelchair is equipped with advanced sensors and navigation systems that allow it to navigate and maneuver autonomously. Users can control the wheelchair through a user-friendly interface, enabling them to move seamlessly.

**4.2 Fall Detection System:** The fall detection system utilizes a combination of accelerometers and gyroscopes to monitor the wheelchair's orientation and detect sudden changes that may indicate a fall. In the event of a fall, the system triggers an alert.

**5. Technical Specifications:**

**5.1 Sensors:**

**HC-SR04 Ultrasonic Sensor:**

**1. Overview:** The HC-SR04 is an ultrasonic ranging module that is widely used for measuring distances without direct contact. It utilizes ultrasonic waves to determine the distance between the sensor and an object.

**2. Key Features:**

* **Ultrasonic Transducer:** The sensor consists of an ultrasonic transducer that emits ultrasonic waves and a receiver that detects the reflected waves.
* **Distance Measurement:** It calculates the distance by measuring the time taken for the ultrasonic waves to travel to the object and back.
* **Wide Range:** The HC-SR04 can measure distances from 2 cm to 400 cm accurately.
* **Easy to Use:** It has a simple interface and requires only a few GPIO pins to operate.

**3. Operating Principle:**

* The HC-SR04 emits a short ultrasonic pulse.
* The pulse travels through the air and hits an object.
* The sensor then listens for the echo of the pulse.
* The time taken for the round trip of the ultrasonic pulse allows the calculation of the distance to the object.

**4. Pin Configuration:**

* **VCC:** Power supply (5V)
* **Trig (Trigger):** Input for triggering the sensor
* **Echo:** Output for receiving the echo signal
* **GND:** Ground

**5. Interface and Usage:**

* To measure distance, a microcontroller (e.g., Arduino) triggers the sensor by sending a pulse to the Trigger pin.
* The Echo pin then outputs a pulse whose duration is proportional to the distance.
* The microcontroller measures this pulse duration to calculate the distance.

**6. Applications:**

* Distance measurement for robotics and automation.
* Object detection and avoidance in various projects.
* Proximity sensing for security systems.
* Liquid level detection in tanks.

**7. Considerations:**

* Accuracy may be affected by the type of surface and environmental conditions.
* Ensure a clear line of sight between the sensor and the object.
* **SW 420 VIBRATION SENSOR**

**1. Sensor Overview:** The SW-420 vibration sensor module typically includes a vibration-sensitive component, a potentiometer for sensitivity adjustment, and an output signal that changes in response to detected vibrations.

**2. Key Features:**

* **Vibration Detection:** The sensor is designed to detect vibrations and shocks.
* **Sensitivity Adjustment:** It often comes with a potentiometer that allows users to adjust the sensitivity of the sensor to better suit the application.
* **Digital Output:** The module typically provides a digital output signal that changes state when vibrations are detected.

**3. Operating Principle:**

* The sensor module contains a vibration-sensitive component that reacts to physical movement.
* When vibrations or shocks occur, the sensor's internal components respond, leading to a change in the output signal.
* The sensitivity can be adjusted using the potentiometer.

**4. Pin Configuration:**

* **VCC:** Power supply (connects to a positive voltage source).
* **GND:** Ground (connects to the ground of the circuit).
* **DO (Digital Output):** Digital signal output that changes state when vibrations are detected.
* **AO (Analog Output):** Some versions may have an analog output providing a variable voltage based on vibration intensity.

**5. Interface and Usage:**

* Connect VCC and GND to the appropriate power supply.
* Connect the DO pin to a digital input on a microcontroller or other digital circuit.
* Adjust the sensitivity using the potentiometer as needed.
* When vibrations are detected, the DO pin will change state, signaling the occurrence of a vibration event.

**6. Applications:**

* Security systems for detecting unauthorized access or tampering.
* Industrial applications for monitoring equipment vibrations.
* Alarms and alert systems triggered by vibrations.
* Home automation projects for detecting movement or activity.

**7. Considerations:**

* Calibration: Adjust the sensitivity according to the specific requirements of the application.
* Mounting: Proper mounting and positioning can impact the sensor's performance.
* Power Supply: Ensure a stable and appropriate power supply for reliable sensor operation.

**5.3 Power System:**

* Long-lasting rechargeable batteries.
* Smart charging system to optimize battery life.

**6. Benefits:**

**6.1 Safety:** The fall detection system significantly reduces the risk of injuries by providing immediate assistance in the event of a fall.

**6.2 Independence:** Users gain greater independence and confidence in their mobility, knowing that the wheelchair is equipped to handle emergencies.

**6.3 Peace of Mind:** Caregivers and family members experience peace of mind, knowing that the automated wheelchair prioritizes user safety.

**7. Challenges and Considerations:** While the automated wheelchair with fall detection offers substantial benefits, there are considerations such as privacy concerns, system reliability, and the need for regular maintenance.

**8. Conclusion:** The integration of fall detection technology in automated wheelchairs represents a significant advancement in assistive technology. By prioritizing user safety and providing timely assistance, these wheelchairs contribute to an improved quality of life for individuals with limited mobility.

**9. Recommendations:** Continued research and development should focus on refining fall detection algorithms, improving system reliability, and addressing user feedback to further enhance the performance and user experience of automated wheelchairs with fall detection capabilities.

**10. Future Outlook:** As technology continues to evolve, the integration of artificial intelligence and machine learning may further enhance the capabilities of automated wheelchairs, making them even more adaptive and responsive to users' needs.

**11. Acknowledgments:** This report acknowledges the contributions of researchers, engineers, and healthcare professionals involved in the development and implementation of automated wheelchairs with fall detection technology. Their dedication to improving the lives of individuals with limited mobility is commendable.

CREDITS:

* 1. SHUBHAM YADAV – PROJECT LEAD
  2. ANKIT JHA – PRESENTATION AND PLANNING
  3. SAGAR YADAV – PLANNING AND ASSEMBLY
  4. DIVYANSH - DESIGINING
  5. THAKUR UDAY – EXECUTION AND CODING